AXAF COMMAND ACTION PROCEDURE

CAP #: 502 ORIGINATOR: Plucinsky DATE: 6 November 1999 COMMANDS CHECKED BY: Time of CAP Execution (GMT): 1999:331:15:00 Last Time of CAP Execution (GMT): 1999:312:22:00

DESCRIPTION/RATIONALE

This CAP contains two ACIS SW command packets which clear and read the static portion of FEP memory Peter is using to store the diagnostic information for the FEP0 bias parity errors. The ACIS operator may choose to execute a read/clear/read (the 1st command, the 2nd command, followed by the first command again) or a read/clear (the 1st and 2nd command) or just simply a read (only the 1st command).

RESTRICTIONS/WARNINGS/NOTES/SCHEDULE REQT:

STEP INSTRUCTIONS (Command/Script) RESPONSE (TLM Verifier) 1 Uplink Loads:

1A RF007 199.CLD D0270BB 1A WF000 140.CLD A0496F9 2 Enable and Activate SCS 199 RF0BPSTACK (command ID = 2155) 3 ACIS confirms receipt of command 4 Enable and Activate SCS 140, if necessary WF0CLSTACK (command ID = 2152) 5 ACIS confirms receipt of command 6 Enable and Activate SCS 199, if necessary RF0BPSTACK (command ID = 2155) 7 ACIS confirms receipt of command 8 Clear and Disable SCSs 140 and 199

Approved:

Subsystem Engineer: Flight Director: TST Manager/Lead: Program Manager: SOT Lead: