AXAF COMMAND ACTION PROCEDURE

CAP #: 517 ORIGINATOR: Plucinsky DATE: 24 November 1999 COMMANDS CHECKED BY: Time of CAP Execution (GMT): 1999:331:14:00

DESCRIPTION/RATIONALE

This CAP executes the SOP which loads the Standard Rev A, Optional Rev A and the FEP0 bias parity error patches. Since ACIS is expected to end an Event Histogram science run in FMT1 at 331:14:20, this CAP switches the spacecraft to FMT2 for 6 minutes in order to clear out the ACIS TLM stream.

RESTRICTIONS/WARNINGS/NOTES/SCHEDULE REQT:

This commanding will be interleaved upon the daily load. There should be no potential conflicts except with ACIS, but the operators should be cognizant nevertheless. The FMT changes have been specified so as not to impact the ongoing HRC observations.

The new command loads for this SW patch are reviewed in ACIS ECO #36-1014.

STEP INSTRUCTIONS (Command/Script) RESPONSE (TLM Verifier) 1 If necessary, stop the current science run 1a Uplink load, 1A AA000 191.CLD 502066E 1b Enable and Activate SCS 191 stopScience (command ID = 1539) 1c If necessary, execute step 1b again 2 switch to FMT 2 at 331:14:21 IMMEDIATELY 3 switch to FMT 1 at 331:14:26 IMMEDIATELY 4 Execute SOP 61082 SW FEP0ENG 5 ACIS confirms ACIS has booted with the

correct flight SW version number. 6 Execute SOP 61010 DEA HKP 7 ACIS confirms existence of DEA HKP data 8 Execute CAP 502 9 Clear and Disable SCS 191 if necessary

Approved:

Subsystem Engineer: Flight Director: TST Manager/Lead: Program Manager: SOT Lead: