AXAF COMMAND ACTION PROCEDURE

CAP #: 528 ORIGINATOR: Plucinsky DATE: 15 Dec 1999 COMMANDS CHECKED BY: Time of CAP Execution (GMT): 354:16:30

DESCRIPTION/RATIONALE

Set the ACIS FP temperature to -125 C approximately 8 hours before the CTI measurements are executed by the daily load at 355:02:30. Reset the FP temperature to -110 C at 335:06:00 after the CTI measuremants have been completed.

RESTRICTIONS/WARNINGS/NOTES/SCHEDULE REQT:

The focal plane temperature will drop very slowly from -110 C to -125 C; nevertheless it should be monitored at least once every two hours. This monitoring requires FMT 1 or 2.

STEP INSTRUCTIONS (Command/Script) RESPONSE (TLM Verifier) 1 Uplink Load:

1A WS033 249.CLD 93705CC 2 Enable and Activate SCS 249 WSFTNEG126 (command ID = 1223) 3 ACIS confirms FP temperature is dropping 4 clear and disable SCS 249 5 Switch to FMT 4 for Continuous Dither Test 6 Switch to FMT 1or2 once every 1-2 hrs

to monitor the FP temperature 7 Daily load executes CTI measurements 8 At 355:06:00, uplink load:

9 1A WS029 255.CLD 7369BB7 10 Enable and Activate SCS 255 WSFTNEG110 (command ID = 741) 11 ACIS confirms FP Temperature is rising 12 Clear and Disable SCS 255

Approved:

Subsystem Engineer: Flight Director: TST Manager/Lead: Program Manager: SOT Lead: