AXAF COMMAND ACTION PROCEDURE

CAP #:544 ORIGINATOR: Plucinsky DATE: 13 Jan 2000 COMMANDS CHECKED BY: Time of CAP Execution (GMT): 015:15:30

DESCRIPTION/RATIONALE

Set the ACIS FP temperature to -110 C as quickly as possible. CAP 543 sets the focal plane to -110 C without turning on the focal plane bakeout heater in 1hr 20min. This CAP uses the focal plane bakeout heater so that the temperature will rise much faster. We will only use this CAP if the COM is poor and we have less time than expected.

RESTRICTIONS/WARNINGS/NOTES/SCHEDULE REQT:

This commanding will be interleaved upon the daily load. There should be no potential conflicts except with ACIS, but the operators should be cognizant nevertheless.

STEP INSTRUCTIONS (Command/Script) RESPONSE (TLM Verifier) 1 Uplink Loads:

1A WB001 194.CLD 7071BA6 1A WS002 195.CLD 4523729 1A WS029 255.CLD 7369BB7 2 Send the following commands:

BUFFER CLEAR ALL BUFFER COMMAND 1WRMBTSB 1WRMBTS1=0 BUFFER SEND VERIFY BUFFER CLEAR ALL 3 Enable and Activate SCS 194 WBBOEN ENB (command ID = 101) 4 ACIS confirms 5 Enable and Activate SCS 195 WSBAKENABL (command ID = 114) 6 ACIS confirms 7 Enable and Activate SCS 255 WSFTNEG110 (command ID = 741) 8 ACIS confirms FP temperature is rising,

takes ¸ 20 minutes 9 Uplink Loads:

1A WS001 205.CLD 6524119 1A WB000 204.CLD 50715A6 1A WD000 137.CLD 8A158A7 1A XD000 185.CLD 4022F12 1A RS000 207.CLD 4022412 10 Enable and Activate SCS 205 WSBAKDSABL (command ID = 116) 11 ACIS confirms 12 Enable and Activate SCS 204 WBBOEN DIS (command ID = 99) 13 ACIS confirms

14 Send the following commands:

BUFFER COMMAND 1WRMBTSB 1WRMBTS1=1 BUFFER SEND VERIFY BUFFER CLEAR ALL 15 Send the following command:

BUFFER COMMAND 1RSETIRT 1RSETIR1 = 1 BUFFER SEND VERIFY BUFFER CLEAR ALL 16 Send the following command:

BUFFER COMMAND 1RSETIRT 1RSETIR1 = 0 BUFFER SEND VERIFY BUFFER CLEAR ALL 17 ACIS confirms that ACIS reboots properly 18 Enable and Activate SCS 137 WD00001024 (command ID = 225) 19 ACIS confirms 20 Enable and Activate SCS 185 XDZ0000005 (command ID = 18) 21 ACIS confirms 22 Clear and Disable 194, 195, 255, 205, 204, 137, 185, and 207

Approved:

Subsystem Engineer: Flight Director: TST Manager/Lead: Program Manager: SOT Lead: