AXAF COMMAND ACTION PROCEDURE

CAP #: 548 ORIGINATOR: Plucinsky DATE: 26 Jan 2000 COMMANDS CHECKED BY: Time of CAP Execution (GMT): 2000:029:22:00

DESCRIPTION/RATIONALE

Set the ACIS FP temperature to -121 C to achieve an actual temperature of -120 C. This is hopefully the final operating temperature of the instrument.

RESTRICTIONS/WARNINGS/NOTES/SCHEDULE REQT:

This commanding will be interleaved upon the daily load. There should be no potential conflicts except with ACIS, but the operators should be cognizant nevertheless.

STEP INSTRUCTIONS (Command/Script) RESPONSE (TLM Verifier) 1 Uplink load:

1A WS032 249.CLD 63705D1 2 Enable and Activate SCS 249 WSFTNEG121 (command ID = 1220) 3 ACIS confirms FP Temperature is dropping 4 Clear and Disable SCS 249

Approved:

Subsystem Engineer: Flight Director: TST Manager/Lead: Program Manager: SOT Lead: