AXAF COMMAND ACTION PROCEDURE

CAP #:616 ORIGINATOR: Plucinsky DATE: 8 June 2000 COMMANDS CHECKED BY: Time of CAP Execution (GMT): 2000:160:21:00

DESCRIPTION/RATIONALE

Perform an ACIS CTI measurement on the ACIS-S array in 3x3 Faint mode.

RESTRICTIONS/WARNINGS/NOTES/SCHEDULE REQT:

This CAP assumes that the spacecraft is in FMT 2.

STEP INSTRUCTIONS (Command/Script) RESPONSE (TLM Verifier) 1 Uplink Loads:

1A WS007 164.CLD 7021872 1A WS00F 233.CLD A03BC6B 1A AA000 191.CLD 502066E 1A XT000 190.CLD C421014 1A RS000 207.CLD 4022412 1A RH000 151.CLD 601EE12 1A WT048 137.CLD 1481FD6 2 Enable and Activate SCS 191, if necessary stopScience (command ID = 1539) 3 Change OBSID to 62882 4 Verify spacecraft in TLM FMT 2 5 Enable and Activate SCS 164 WSVIDALLDN (command ID = 1541) 6 Enable and Activate SCS 233 WSPOW3F03F (command ID = 360) 7 Enable and Activate SCS 137 WT0021C014 (command ID = 2046) 8 Enable and Activate SCS 190 XTZ0000005 (command ID = 58) 9 Enable and Activate SCS 207 RS 0000001 (command ID =66) 10 Enable and Activate SCS 151 RH 0000001 (command ID = 68) 11 ACIS confirms science run is progressing

nominally as time permits 12 Clear and Disable SCSs 190,191,164,233,207,151,137

Approved:

Subsystem Engineer: Flight Director: TST Manager/Lead: Program Manager: SOT Lead: