AXAF COMMAND ACTION PROCEDURE

CAP # 626 Rev A ORIGINATOR: Paul Plucinsky DATE: 28 June 2000 COMMANDS CHECKED BY: Time of CAP Execution (GMT): 180:22:10

DESCRIPTION/RATIONALE

This CAP is a response to the anomalies seen in OBSIDs 371, 659, and 861. FEP 0 and FEP 3 appear to be reporting a high number of anomalous events. This CAP will be executed in place of the planned Squeegy run of CAP 625.

The plan is:

ffl Dump Flight SW

ffl Dump volatile memory, steps 1-4,5L-5W,7L, & 10 of SOP 61024

ffl Power down the FEPs, WSFEPALLDN

ffl Warm Boot the BEP, SOP 61070

ffl execute normal CTI I array (rerun of CAP 574)

RESTRICTIONS/WARNINGS/NOTES/SCHEDULE REQT:

STEP INSTRUCTIONS (Command/Script) RESPONSE (TLM Verifier) EXECUTE:

1 Uplink Load

1A RB000 196.CLD 40E372D 2 Enable and Activate SCS 196 RBROMDUMP1 (cmdId = 306) 3 Disable and clear SCS 196 4 execute steps 1-4,5L-5W,7L,10 of SOP 61024 ACIS verifies 5 Uplink Load

1A WS003 165.CLD 8121972 6 Enable and Activate SCS 165 WSFEPALLDN (cmdId = 1542) 7 clear and disable SCS 165 8 SOP 61070 Warm Boot ACIS verifies 9 SOP 61010 Start DEAHkp ACIS verifies 10 CAP 574 ACIS CTI on I array ACIS verifies

Approved:

Subsystem Engineer: Flight Director: TST Manager/Lead: Program Manager: SOT Lead: