AXAF COMMAND ACTION PROCEDURE

CAP # 626 Rev B ORIGINATOR: Paul Plucinsky DATE: 29 June 2000 COMMANDS CHECKED BY: Time of CAP Execution (GMT): 181:00:58

DESCRIPTION/RATIONALE

This CAP is the AS-RUN version of CAP 626. See CAP 626 Rev A for the intention of the CAP. Due to problems with the Squirt connection to the EGSE and the poor COM on Madrid, CAP 626 had to be truncated. See SOT shift report Jun 28 2000 H342.txt for additional details.

The plan is:

ffl Power down the FEPs, WSFEPALLDN

ffl Dump Flight SW

ffl execute normal CTI I array (rerun of CAP 574)

RESTRICTIONS/WARNINGS/NOTES/SCHEDULE REQT:

STEP INSTRUCTIONS (Command/Script) RESPONSE (TLM Verifier) EXECUTE:

1 Uplink Load 180:22:30

1A RB000 196.CLD 40E372D 2 switch to DSS 24 181:00:50 3 Uplink Load 181:01:05

1A WS003 165.CLD 8121972 4 Enable and Activate SCS 165 181:01:06 WSFEPALLDN (cmdId = 1542) 5 clear and disable SCS 165 181:01:07 6 Uplink Load 181:01:09

1A CTI00 137.CLD 181:01:10 E1940CB 7 Enable and Activate SCS 137 181:01:10 WSVIDALLDN (command ID = 1541) WSPOW0CF3F (command ID = 359) RS 0000001 (command ID = 66) RH 0000001 (command ID = 68) WT00216014 (command ID = 2034 ) 8 ACIS confirms XTZ0000005 (command ID = 58) 9 Enable and Activate SCS 196 181:01:17 RBROMDUMP1 (cmdId = 306) 10 Disable and clear SCS 196 181:01:25 11 Clear and Disable 137 181:01:39 12 LOS on DSS 24 181:01:46

Approved:

Subsystem Engineer: Flight Director: TST Manager/Lead: Program Manager: SOT Lead: