AXAF COMMAND ACTION PROCEDURE

CAP #: 634 ORIGINATOR: Plucinsky DATE: 11 July 2000 COMMANDS CHECKED BY: Time of CAP Execution (GMT): 2000:196:03:30

DESCRIPTION/RATIONALE

This CAP executes what were to be steps 22,23,24,25,26,38,39, & 40 of CAP625B. We ran CAP625B in the low radiation period during the large radiation storm on day 195. Therefore, it is best to run this CAP to stop the on-going Squeegy run and claen-up ACIS before the interrupt load starts running.

RESTRICTIONS/WARNINGS/NOTES/SCHEDULE REQT:

This commanding will be interleaved upon the daily load. There should be no potential conflicts except with ACIS (see discussion above), but the operators should be cognizant nevertheless.

STEP INSTRUCTIONS (Command/Script) RESPONSE (TLM Verifier) 1 Uplink Loads:

1A AA000 191.CLD 502066E 1A RYFS0 211.CLD F423E81 1A RZFS0 217.CLD 4424581 1A W2011 159.cld DE51504 2 Enable and Activate SCS 191 ¸ 196 : 04 : 00 stopScience (cmdId = 1539) 3 ACIS confirms normal completion of science run 4 Enable and Activate SCS 211 readPram (cmdId = 1613) 5 ACIS confirms receipt of PRAM dump 6 Enable and Activate SCS 217 readSram (cmdId = 1602) 7 ACIS confirms receipt of SRAM dump 8 Enable and Activate SCS 159 load2dBlock, W200038014 (cmdId = 2141) 9 Clear and Disable SCSs 191, 211, 217, 159

Approved:

Subsystem Engineer: Flight Director: TST Manager/Lead: Program Manager: SOT Lead: