\documentstyle[11pt]{article}

\topmargin -1.00truein
\oddsidemargin -0.5truein
\textheight 10.0truein
\textwidth 6.7truein


\begin{document}


\begin{table}[th]
\centering
\caption[ ]{\bf Paul's Status of AXAF FLIGHT ACIS COMMAND SEQUENCES}


\begin{tabular}{|l|l|c|}
\hline
\hline
ORBITAL ACTIVIATION PROCEDURES & &  \\
\hline
TITLE 								& FILE
NAME &STATUS \\
\hline
							        & &		\\ 
SHUTTLE PHASE							& &		\\
							        & &		\\
Open Little Vent Valve (Realtime Version)			&
open\_lvv.$\ast$ & I \\
							        & &		\\
\hline
TRANSFER ORBIT							& &		\\
\hline
							        & &		\\
Monitor Temperatures and Pressure During Orbital Insertion	&
monitor\_tp.$\ast$  & I \\
Turn on DPA A \& B and DEA A [realtime version]			& turnon\_dpaab\_deaa.$\ast$ & I \\
Load DEA HK PB and Start DEA HK run				&
deahkp.$\ast$ & I \\
Turn on DA Heater side B					&
dahtr\_b\_on.$\ast$ & I \\
Set focal plane temperature to -120 C				&
setFP\_m120.$\ast$ & I \\
Open Large Vent Valve						&
open\_vv.$\ast$ & D \\
Partial Bakeout, set FP to -50 C				&
bakeout\_m50C.$\ast$ & N \\
Set focal plane temperature to -90 C				&
setFP\_m90.$\ast$ & D \\
Dump flight SW							&
fs\_dump.$\ast$ & I \\
Flight Software Standard Set of Patches				&
sw\_stdpatch.$\ast$ & UD \\
Flight Software Event Histogram and CC 3x3 Patch		&
sw\_optevhcc3x3.$\ast$ & UD \\
Flight Software Event Histogram Patch 				&
sw\_evhpatch.$\ast$ & I \\
Diagnostic Mode							&
ccd\_diag\_posttv.$\ast$ & I \\
Raw Data from each CCD						&
ccd\_raw.$\ast$ & I \\
OBF Integrity Test						&
ccd\_obf.$\ast$  & PB \\
Dark Current Measurement					&
ccd\_dark.$\ast$ & PB \\
Internal Calibration Source Measurement at -90~C		&
ccd\_int1.$\ast$ & PB \\
Internal Calibration Source Measurement at -110~C		&
ccd\_int2.$\ast$ & PB \\
Internal Calibration Source Measurement at -120~C		&
ccd\_int3.$\ast$ & PB \\
Event Histogram on the Internal Cal Source with ACIS-S in Fmt 1 &
ccd\_evhist\_s.$\ast$ & I \\
							        & &	\\
\hline
ABRIDGED LONG FORM FUNCTIONAL TEST				& &		\\
\hline
							        & &		\\
Diagnostic Mode							&
ccd\_diag\_posttv.$\ast$ & I \\
Exercise Detector Housing Heater Controls			&
heater\_fp.$\ast$ & O \\
Software Boot Modes: Uplink					&
uplink\_boot.$\ast$ & I \\
Software Boot Modes: Warm \& Cold				&
swbootmode.$\ast$ & I \\
BEP/DEA Power Combinations					&
power\_combo.$\ast$ & I \\
DEA/FEP MUX Verification					&
deafep\_mux.$\ast$ & I \\
Set DACs Low and High						&
dac\_limits.$\ast$ & O \\
							        & &	\\
\hline
FINAL ORBIT							& &	\\
\hline
							        & &  \\
Characterize Background before opening ACIS door		&
ccd\_orbbkg1.$\ast$  & PB \\
Full Bakeout							&
full\_bakeout.$\ast$ & D \\
Open ACIS Camera Housing Door					&
open\_door\_4shots.$\ast$  & D \\
Characterize Background after opening ACIS door			&
ccd\_orbbkg2.$\ast$ & PB \\
							        & & \\
\hline

\end{tabular}

\end{table}


\begin{table}[th]
\centering
\caption[ ]{\bf Paul's Status of AXAF FLIGHT ACIS COMMAND SEQUENCES}

\begin{tabular}{|l|l|c|}
\hline
TITLE 								&
FILENAME & STATUS \\
\hline
\hline
HRMA ACC OPENS							& & \\
\hline
							        & &  \\
HRMA Flux Transfer Standard Sources Measurements		&
ccd\_fcm.$\ast$  & PB  \\
							        & & \\
\hline
HRMA SUNSHADE DOOR OPENS					& & \\
\hline
							        & & \\
Phase II activities commanded through ORs			& &  \\
							        & & \\
							        & & \\
\hline
ACIS STORED COMMAND SEQUENCES					& & \\
\hline
							        & & \\
Load Shed Procedure SCS 40					& NA & NA \\
Autonomous power-up SCS 70					& NA & NA \\
							        & & \\
\hline
ACIS ``ATOMIC'' PROCEDURES					& &		\\
\hline
							        & &		\\
Turn on DPA A \& B and DEA A [realtime version]			&
turnon\_dpaab\_deaa.$\ast$ & I \\
Turn on DPA A \& B and DEA A [SCS version]			&
turnon\_dpaab\_deaa\_scs.$\ast$ & I \\
Turn on DPA A (TSV)						&
turnon\_dpaa.$\ast$ & O \\
Turn on DPA B (TSV)						&
turnon\_dpab.$\ast$ & O \\
Turn on DEA A (TSV)						&
turnon\_deaa.$\ast$ & O \\
Turn off DPA A (TSV)						&
turnoff\_dpaa.$\ast$  & O \\
Turn off DPA B (TSV)						&
turnoff\_dpab.$\ast$ & O \\
Turn off DEA A (TSV)						&
turnoff\_deaa.$\ast$ & O \\
Turn off DPA A \& B and DEA A (TSV)				&
turnoff\_dpaab\_deaa.$\ast$ & I \\
Put ACIS into memory save mode for eclipse			&
mem\_save.$\ast$ & I \\
Put ACIS into standy mode for eclipse				&
standby.$\ast$ & I \\
Load DEA HK PB and Start DEA HK run				&
deahkp.$\ast$  & I \\
Turn on DA Heater side B					&
dahtr\_b\_on.$\ast$ & I \\
Set focal plane temperature to -120 C				&
setFP\_m120.$\ast$ & I \\
Set focal plane temperature to -50 C (TSV)			&
setFP\_m50.$\ast$ & N \\
Set focal plane temperature to -90 C (TSV)			& setFP\_m90.$\ast$ & D \\
Warm Boot the ACIS BEP						&
warmboot.$\ast$ & N \\
Cold Boot the ACIS BEP						&
coldboot.$\ast$ & N		\\
\hline

\end{tabular}


\end{table}




\begin{table}[th]

\centering
\caption[ ]{\bf Paul's Status of AXAF FLIGHT ACIS COMMAND SEQUENCES}

\begin{tabular}{|l|l|c|}
\hline
TITLE 								& FILENAME & STATUS \\
\hline
\hline
ACIS CONTINGENCY PROCEDURES					& &		\\
\hline
							        & &		\\
Open Little Vent Valve for emergency deployment (SCS Version)	&
open\_lvv\_emgdep.$\ast$ & N \\
Close Little Vent Valve						&
close\_lvv.$\ast$ & O \\
Abort Opening Large Vent Valve					&
abort\_opvv.$\ast$ & O  \\
Close Large Vent Valve						&
close\_vv.$\ast$ & O \\
Abort Closing Large Vent Valve					&
abort\_clvv.$\ast$ & O  \\
Turn Off DA heater side B and turn on side A 			& dahtr\_aon\_boff.$\ast$ & N \\
Turn Off DA heater side A and turn on side B 			&
dahtr\_bon\_aoff.$\ast$ & N \\
Switch from BEP A to BEP B       				&
switch\_bepa\_b.$\ast$ & N \\
Switch from DEA A to DEA B       				&
switch\_deaa\_b.$\ast$ & N \\

\hline


\end{tabular}

\raggedright
{\bf {\noindent Classification scheme:}} \\
{\noindent I: version on Paul's flight web page is identical to
version which was used to generate ground test procedure, no
modification to existing FOT procedure should be necessary} \\
{\noindent N: new procedure since EST II test on 12/99 } \\
{\noindent D: procedure has been modified from ground testing version} \\
{\noindent O: old procedure, available on the web page for many months
but not developed by the FOT.} \\
{\noindent UD: procedure is still under development, mostly PBs and
new contingency procedures} \\

\vspace{0.2in}
{\bf NOTE: all files located in ``/home/plucinsk/www/cmd\_seq''}

\end{table}




\end{document}
