\documentclass[11pt]{article}

\usepackage{lscape}

\topmargin -0.90truein
\oddsidemargin -0.75truein
\textheight 10.0truein
\textwidth 7.0truein
\hbadness=10001
\hfuzz=200pt

\thispagestyle{empty}
\setcounter{table}{1}

\begin{document}


\begin{landscape}

\begin{table}[tbp]
\centering
\caption[ ]{\bf FOT Flight Procedure Release on March 19, 1999}

\begin{tabular}{|l|l|l|l|c|}
\hline
\#  & Title		& Filenames & SOP name & New PB \\
\hline
\hline
          & NOT FLIGHT PROCEDURES & & & \\
          & Update Bad Pixel and Column List & update\_bad & MZ\_61018\_BAD\_PIXEL\_ppp.txt & \\
          & Killer Patch  & sw\_patch & MZ\_61003\_FLT\_SWP\_ppp.txt & \\  
     & Flight Software Standard Set of Patches (SCS)  & sw\_stdpatch & MZ\_61004\_FLT\_SWSP\_ppp.txt & \\
     & Diagnostic Mode [realtime version] & ccd\_diag\_posttv & MZ\_61001\_DIAG\_RTL\_ppp.txt &  \\
\hline
          & SHOULD BE A FLIGHT PROCEDURE  & & & \\
4.19\_V1.1 & Radiation Belt Entry  & radbelt\_entry & MZ\_61020\_RAD\_BELT\_ENTRY\_ppp.txt & \\
 \hline
1.8\_V1.1 & Partial Bakeout, set FP to -50 C & bakeout\_m50C & MZ\_61056\_PBO\_NEG50\_ppp.txt & \\
\hline
1.11\_V1.1 & Flight Software Standard Set of Patches (realtime) & sw\_stdpatch & MZ\_61027\_FLT\_SWSP\_RTL\_ppp.txt & Y \\
\hline
1.12\_V1.1 & Flight Software Event Histogram and CC 3x3 Patch & sw\_optevhcc3x3 & MZ\_61007\_SWP\_HIST\_3x3\_ppp.txt & Y \\
\hline
1.15\_V1.1 & OBF Integrity Test & ccd\_obf & MZ\_61053\_OBF\_INTEGRITY\_ppp.txt & Y \\
\hline
1.16\_V1.1 & Dark Current Measurement & ccd\_dark & MZ\_61052\_DARK\_CUR\_MEAS\_ppp.txt & Y \\
\hline
1.18\_V1.1 &  Internal Calibration Source Measurement at -90~C & ccd\_int1 & MZ\_61051\_INT\_CAL\_MEA\_90\_ppp.txt & Y \\
\hline
1.19\_V1.1  & Internal Calibration Source Measurement at -110~C &
ccd\_int2 & MZ\_61050\_INT\_CAL\_MEA\_110\_ppp.txt & Y \\
\hline
2.2\_V1.1 & Exercise Focal Plane Heater Controls & heater\_fp & MZ\_61048\_EXER\_DH\_HEAT\_CTRL\_ppp.txt & Y \\
\hline
2.7\_V1.1 & DEA Video Board DAC Limit Test & dac\_limits & MZ\_61047\_DACS\_LOW\_HIGH\_ppp.txt & Y \\
\hline
2.8\_V1.1  & CCD Orbital Background Measurements & ccd\_orbbkg1 & MZ\_61046\_CHAR\_BKGRND\_CLOSE\_ppp.txt & Y \\
\hline
2.11\_V1.1 & CCD Orbital Background Measurements II & ccd\_orbbkg2 & MZ\_61045\_CHAR\_BKGRND\_OPEN\_ppp.txt & Y \\
\hline
2.12\_V1.1  & HRMA Flux Standard Transfer Sources Measurements & ccd\_fcm & MZ\_61044\_FLX\_XFR\_STD\_ppp.txt & Y \\
\hline
4.2\_V1.1  & Turn on DPA A \& B and DEA A [SCS version] & turnon\_dpaab\_deaa\_scs & MZ\_61039\_DPA\_ON\_SCS\_ppp.txt & Y \\
\hline
4.3\_V1.1  & Turn on DPA A  & turnon\_dpaa & MZ\_61038\_DPA\_A\_ON\_ppp.txt & \\
\hline
4.4\_V1.1  & Turn on DPA B  & turnon\_dpab & MZ\_61037\_DPA\_B\_ON\_ppp.txt & \\
\hline
4.5\_V1.1  & Turn on DEA A  & turnon\_deaa & MZ\_61036\_DEA\_A\_ON\_ppp.txt & \\
\hline
4.6\_V1.1  & Turn off DPA A & turnoff\_dpaa & MZ\_61035\_DPA\_A\_OFF\_ppp.txt & \\
\hline
4.7\_V1.1  & Turn off DPA B & turnoff\_dpab & MZ\_61034\_DPA\_B\_OFF\_ppp.txt & \\
\hline
4.8\_V1.1  & Turn off DEA A & turnoff\_deaa & MZ\_61033\_DEA\_A\_OFF\_ppp.txt & \\
\hline
4.15\_V1.1 & Set focal plane temperature to -50 C & setFP\_m50 & MZ\_61059\_FPTEMP\_NEG50\_ppp.txt & \\
\hline
4.17\_V1.1 & Warm Boot the ACIS BEP & warmboot & MZ\_61070\_WARM\_BOOT\_ppp.txt & \\
\hline
4.18\_V1.1 & Cold Boot the ACIS BEP & coldboot & MZ\_61071\_COLD\_BOOT\_ppp.txt & \\
\hline
5.1\_V1.1 & Close Little Vent Valve & close\_lvv & MZ\_51000\_CLOSE\_lvv\_ppp.txt      & \\
\hline
5.2\_V1.1 & Abort Opening Large Vent Valve & abort\_opvv & MZ\_51001\_ABORT\_OPEN\_LVV\_ppp.txt & \\
\hline
5.3\_V1.1 & Close Large Vent Valve & close\_vv & MZ\_51002\_LRGVV\_CLOSE\_ppp.txt
\hline
  & \\
\hline
5.4\_V1.1 & Abort Closing Large Vent Valve & abort\_clvv &  MZ\_51003\_ABORT\_CLOSING\_LVV\_ppp.txt & \\
\hline
5.5\_V1.1 & Open Little Vent Valve in Emergency Deployment  & open\_lvv\_emgdep & MZ\_51004\_OPEN\_LVV\_DEPLOY\_ppp.txt & \\
          & [SCS version] & & & \\
\hline
5.6\_V1.1 & Turn Off DA heater side B and turn on side A & dahtr\_aon\_boff & MZ\_51005\_DAHTR\_B\_TO\_A\_ppp.txt & \\
\hline
5.7\_V1.1 & Turn Off DA heater side A and turn on side B & dahtr\_bon\_aoff & MZ\_51006\_DAHTR\_A\_TO\_B\_ppp.txt & \\
\hline
5.8\_V1.1 & Switch from BEP A to BEP B & switch\_bepa\_b & MZ\_51007\_BEP\_A\_TO\_B\_ppp.txt &  \\
\hline
5.9\_V1.1 & Switch from DEA A to DEA B & switch\_deaa\_b & MZ\_51008\_DEA\_A\_TO\_B\_ppp.txt & Y \\
\hline
\end{tabular}

\end{table}

\end{landscape}

\end{document}

