\documentclass[11pt]{article}

\usepackage{lscape}

\topmargin -0.75truein
\oddsidemargin -0.4truein
\textheight 9.25truein
\textwidth 6.7truein
\hbadness=10001
\hfuzz=200pt


\begin{document}
%\input dspace12.tex
%\input pstricks.tex
%\input psfig
\newcommand{\be}{\begin{enumerate}}
\newcommand{\ee}{\end{enumerate}}
\newcommand{\bc}{\begin{center}}
\newcommand{\ec}{\end{center}}
\newcommand{\bi}{\begin{itemize}}
\newcommand{\ei}{\end{itemize}}
\newcommand{\bd}{\begin{description}}
\newcommand{\ed}{\end{description}}
\newcommand{\bt}{\begin{tabbing}}
\newcommand{\et}{\end{tabbing}}
\newcommand{\eg}{{\it e.g.~}}
\newcommand{\ie}{{\it i.e.~}}
\newcommand{\ul}{\underline}
\newcommand{\axaf}{{\em AXAF}}
\def\la{\hbox{\rlap{$<$}\lower0.5ex\hbox{$\sim$}\ }}


\large
%\vspace*{-0.5in}
\centerline {\bf 1.31\_V2.0 Continuous Clocking Raw Data }
\vspace{0.25in}

\normalsize
\noindent{\it Last Revised: August 6, 1999}\\


\noindent {\bf BRIEF FUNCTIONAL DESCRIPTION:} \\
\normalsize

This procedure will telemeter raw frames in continuous clocking mode
to be used to characterize the effects of particle-induced events on
CC mode bias maps and event processing.  The time required to
telemeter one CC raw frame should be about 2 min.  This procedure will
run for 5 hours and should collect about 15 raw frames from each of
the 10 CCDs.


\vspace{0.25in}
\noindent The sequence of actions will be: 
\be
\item warm boot and start DEA housekeeping if necessary
\vspace{-0.10in}
\item configure the instrument to collect imaging array data
\vspace{-0.10in}
\item execute the continuous clocking 3x3 mode science run
\vspace{-0.10in}
\item configure the instrument to collect spectroscopy array data
\vspace{-0.10in}
\item execute the continuous clocking 3x3 mode science run
\vspace{-0.10in}
\item return to thermal standby mode if necessary
\vspace{-0.10in}
\ee


\vspace{0.15in}
\normalsize
\noindent {\bf ASSUMED INSTRUMENT STATE:} \\
\normalsize
Assumes that the instrument is in the cannonical thermal standby mode. \\
Assumes that the standard patches have been loaded. \\

%\vspace{0.25in}
\normalsize
\noindent {\bf SPECIAL INITIAL CONDITIONS:} \\
\normalsize

The continuous clocking 3x3 optional patch must have been loaded
before this procedure begins. \\

%\newpage 

%\vspace{0.25in}
\normalsize
\noindent {\bf OPERATIONAL CONSTRAINTS/CAUTIONS:} \\
\normalsize


\vspace{0.15in}
\normalsize
\noindent {\bf REFERENCES:} \\
\normalsize

\normalsize
\noindent {\bf CHANGE HISTORY:} \\
\normalsize

{\bf V1.0}
\begin{itemize}

\item Initial version, copied from procedure 1.25\_V2.1, ``Continuous
Clocking 3x3''

\item Revised brief functional description

\item Revised command mnemonics and command echos in steps 3.1, 3.2, 5.1, and
5.2

\item Revised description fields in steps 3.2 and 5.2

\item In steps 3.15 and 5.15, set time requirement fields to ``120
min'', tlm criterion field to ``A'', real time contact field to ``Y'',
and modified the description fields

\item Set time requirement field to ``1 min'' in step 3.16

\item Set real time contact field to ``Y'' in step 5.16

\item Added steps 3.17 and 5.17 to wait ``25 min'' for telemetry to
send down the remaining raw frames after the science run is stopped

\end{itemize}

{\bf V2.0}
\begin{itemize}
\item added SW command mnemonics and command IDs for the PBs and
window blocks in steps 3.1,3.2,5.1, and 5.2
\end{itemize}

\newcommand{\tablecaptiontext}{Continuous Clocking 3x3 Raw Data}
\input{ccraw_data.tab}

\end{document}
