\documentclass[11pt]{article}

\usepackage{lscape}

\topmargin -0.75truein
\oddsidemargin -0.4truein
\textheight 9.25truein
\textwidth 6.7truein
\hbadness=10001
\hfuzz=200pt


\begin{document}
%\input dspace12.tex
%\input pstricks.tex
%\input psfig
\newcommand{\be}{\begin{enumerate}}
\newcommand{\ee}{\end{enumerate}}
\newcommand{\bc}{\begin{center}}
\newcommand{\ec}{\end{center}}
\newcommand{\bi}{\begin{itemize}}
\newcommand{\ei}{\end{itemize}}
\newcommand{\bd}{\begin{description}}
\newcommand{\ed}{\end{description}}
\newcommand{\bt}{\begin{tabbing}}
\newcommand{\et}{\end{tabbing}}
\newcommand{\eg}{{\it e.g.~}}
\newcommand{\ie}{{\it i.e.~}}
\newcommand{\ul}{\underline}
\newcommand{\axaf}{{\em AXAF}}
\def\la{\hbox{\rlap{$<$}\lower0.5ex\hbox{$\sim$}\ }}


\large
%\vspace*{-0.5in}
\centerline {\bf 1.5\_V2.0 TURN ON DA HEATER SIDE B }
\vspace{0.25in}

\normalsize
\noindent{\it Last Revised: June 23,1999}\\
\noindent{\bf Filename: dahtr\_b\_on} \\


\noindent {\bf BRIEF FUNCTIONAL DESCRIPTION:} \\
\normalsize
This is an ``atomic'' procedure which simply turns on the detector
assembly heater side B.  This heater controls the DA housing
temperature to be -60 C.

\vspace{0.25in}
\noindent The sequence of actions will be: 
\be
\item enable and turn on the DA heater side B
\vspace{-0.10in}
\item monitor the Camera Body and Warm Radiator temperature
\ee


\vspace{0.15in}
\normalsize
\noindent {\bf ASSUMED INSTRUMENT STATE:} \\
\normalsize


%\vspace{0.25in}
\normalsize
\noindent {\bf SPECIAL INITIAL CONDITIONS:} \\
\normalsize
%The environment must be clean enough to allow opening of the valve. \\
%Assumes that \axaf\/ ISIM RCTU is powered on and in telemetry format 6. \\

%\newpage 

%\vspace{0.25in}
\normalsize
\noindent {\bf OPERATIONAL CONSTRAINTS/CAUTIONS:} \\
\normalsize



\vspace{0.15in}
\normalsize
\noindent {\bf REFERENCES:} \\
\normalsize

\normalsize
\noindent {\bf CHANGE HISTORY:} \\
\normalsize

{\bf V1.2}
\begin{itemize}
\item added expected values of HW TLM verifiers in step 1.2
\item added step 1.3 to monitor the Camera Body and Warm Radiator's
temperatures
\item added filename identification to top of procedure
\end{itemize}

{\bf V2.0}
\begin{itemize}
\item ACIS Team signed-off version
\item changed ``Assumed Instrument State'' to read nothing
\item changed required TLM FMT to be 1,2,4or6
\item changed comment in ``Description'' column in step 1.2
\end{itemize}

\newcommand{\tablecaptiontext}{TURN ON DETECTOR ASSEMBLY HOUSING HEATER SIDE B}
\input{dahtr_b_on.tab}

\end{document}
