\documentclass[10pt]{article}

\usepackage{lscape}

\topmargin -0.75truein
\oddsidemargin -0.6truein
\textheight 9.75truein
\textwidth 7.0truein
\hbadness=10001
\hfuzz=200pt

\thispagestyle{empty}

\begin{document}


\begin{table}[tbp]
\centering
\caption[ ]{\bf SOT Flight Procedure Signoff}

\begin{tabular}{|l|l|}
\hline
\#  & Title		\\
\hline
\hline
    & ALREADY SIGNED OFF \\
\hline
1.1\_1.5 & Open Small Vent Valve \\
1.7\_V1.5 & Open Big Vent Valve \\
2.10\_V1.4 & Open ACIS Door On Orbit  \\
1.10\_V1.2 & Dump Flight SW \\
\hline
    & COMMENTS BY COB JUNE 22 \\
\hline
1.22\_V1.0 & Turn On Press. XDCRs A \& B \\
4.20\_V1.0 & Turn Off Press. XDCRs A \& B \\
1.3\_V1.5 & Turn on DPA A \& B and DEA A \\
1.4\_V1.4 & Load DEA HK PB and  Start DEA HKP run \\
1.5\_V1.2 & Turn on the DA Heater Side B \\
1.6\_V1.3 & Set FP Temperature to -120~C  \\
1.8\_V1.4 & Partial Bakeout, Set FP to -50~C \\
1.9\_V1.4 & Set FP Temperature to -90 C \\
1.13\_V1.5 & Diagnostic Mode \\
\hline
    & COMMENTS BY COB JUNE 25 \\
\hline
1.11\_V1.2 & Flight SW Standard Patches  \\
1.12\_V1.3 & Flight SW Event Histogram and CC 3x3 Patch \\
1.14\_V1.3 & Raw Data from each CCD \\
1.15\_V1.3 & OBF Integrity Test \\
1.16\_V1.3 & Dark Current Measurement \\
1.23\_V1.0 & Internal Cal Source Meaurement \\
1.21\_V1.3 & Event Histogram on the Int Cal Source with ACIS-S in fmt 1 \\
1.24\_V1.0 & Event Histogram on the Int Cal Source with ACIS-I in fmt 1 \\ 
2.3\_V1.4 & SW Boot Modes: Uplink Boot  \\ 
2.4\_V1.3 & SW Boot Modes: Warm and Cold \\
2.5\_V1.3 & BEP/DEA Power Combinations \\ 
2.6\_V1.3 & DEA/FEP MUX Verification \\ 
5.5\_V1.3 & Open Small Vent Valve in an Emergency Deployment \\
\hline
    & COMMENTS BY COB JULY 2 \\
\hline
2.9\_V1.3 & Full Bakeout \\
2.13\_V1.0 &  Exit Full Bakeout and Return to Thermal Standby Mode \\
2.11\_V1.4 & CCD Orbital Background Meas. with the ACIS Door Open   \\ 
2.12\_V1.3  & HRMA Flux Standard Transfer Sources Measurement \\ 
3.2\_V1.3  & Emergency Load Shed Procedure \\ 
3.4\_V1.3  & Autonomous Power-Up Procedure \\
4.2\_V1.3  & Turn on DPA A \& B and DEA A [SCS version] \\ 
4.3\_V1.3  & Turn on DPA A   \\ 
4.4\_V1.3  & Turn on DPA B  \\
4.5\_V1.3  & Turn on DEA A  \\
4.6\_V1.3  & Turn off DPA A \\
4.7\_V1.3  & Turn off DPA B \\
4.8\_V1.3  & Turn off DEA A \\
4.9\_V1.3 & Turn Off DPA A \& B and DEA A \\
4.10\_V1.2 & Put ACIS into Memory Save Mode \\
4.11\_V1.2 & Put ACIS into Standby Mode  \\ 
4.17\_V1.2 & Warm Boot the ACIS BEP \\
4.18\_V1.2 & Cold Boot the ACIS BEP \\
4.19\_V1.2 & Radiation Belt Entry  \\ 
4.21\_V1.0 & Set FP Temperature to -110~C  \\
5.1\_V1.3 & Close Small Vent Valve \\
5.3\_V1.4 & Close Big Vent Valve  \\ 
5.6\_V1.2 & Turn Off DA heater side B and turn on side A  \\
5.7\_V1.2 & Turn Off DA heater side A and turn on side B \\ 
5.8\_V1.3 & Switch from BEP A to BEP B \\
5.9\_V1.2 & Switch from DEA A to DEA B \\
\hline
\end{tabular}

\end{table}



\end{document}

