\documentclass[11pt]{article}

\usepackage{lscape}

\topmargin -0.75truein
\oddsidemargin -0.4truein
\textheight 9.25truein
\textwidth 6.7truein
\hbadness=10001
\hfuzz=200pt


\begin{document}
%\input dspace12.tex
%\input pstricks.tex
%\input psfig
\newcommand{\be}{\begin{enumerate}}
\newcommand{\ee}{\end{enumerate}}
\newcommand{\bc}{\begin{center}}
\newcommand{\ec}{\end{center}}
\newcommand{\bi}{\begin{itemize}}
\newcommand{\ei}{\end{itemize}}
\newcommand{\bd}{\begin{description}}
\newcommand{\ed}{\end{description}}
\newcommand{\bt}{\begin{tabbing}}
\newcommand{\et}{\end{tabbing}}
\newcommand{\eg}{{\it e.g.~}}
\newcommand{\ie}{{\it i.e.~}}
\newcommand{\ul}{\underline}
\newcommand{\axaf}{{\em AXAF}}
\def\la{\hbox{\rlap{$<$}\lower0.5ex\hbox{$\sim$}\ }}


\large
%\vspace*{-0.5in}
\centerline {\bf 2.16\_1.1  VIDEO BOARD TEMPERATURE MEASUREMENTS }
\vspace{0.25in}

\normalsize
\noindent{\it Last Revised: August 24, 1999}\\


\noindent {\bf BRIEF FUNCTIONAL DESCRIPTION:} \\
\normalsize
This procedure will run a special dea housekeeping run to
collect video board temperatures as Chandra comes out of 
radiation.


\vspace{0.25in}
\noindent The sequence of actions will be: 
\be
\item start DEA housekeeping with video board temperatures
\vspace{-0.10in}
\item configure the instrument to collect imaging array data
\vspace{-0.10in}
\item execute the faint mode science run
\vspace{-0.10in}
\item return to thermal standby mode
\vspace{-0.10in}
\ee


\vspace{0.15in}
\normalsize
\noindent {\bf ASSUMED INSTRUMENT STATE:} \\
\normalsize
Assumes that the instrument is in the cannonical thermal standby mode.
Assumes that the standard patches have been loaded. \\


%\vspace{0.25in}
\normalsize
\noindent {\bf SPECIAL INITIAL CONDITIONS:} \\
\normalsize


%\newpage 

%\vspace{0.25in}
\normalsize
\noindent {\bf OPERATIONAL CONSTRAINTS/CAUTIONS:} \\
\normalsize


\vspace{0.15in}
\normalsize
\noindent {\bf REFERENCES:} \\
\normalsize

\normalsize
\noindent {\bf CHANGE HISTORY:} \\
\normalsize

{\bf V1.0}
Original version.

{\bf V1.1}
\begin{itemize}
\item  Change parameter block loaded in step 3.1 to WT000A8014
\item  Add step to dump the Huffman table, RH\_0000001, at step 3.3.
\item  Increased the wait time in step 3.5 to 60 minutes.
\item  Deleted step 4.2 to power down the FEPs, WSFEPALLDN. 
\end{itemize}


\newcommand{\tablecaptiontext}{Video Board Temperature Measurements}
\input{vid_temp.tab}

\end{document}
