AXAF COMMAND ACTION PROCEDURE

CAP #: 503 ORIGINATOR: Plucinsky DATE: 6 November 1999 COMMANDS CHECKED BY: Time of CAP Execution (GMT): 1999:332:00:35 Last Time of CAP Execution (GMT): 1999:314:06:00

DESCRIPTION/RATIONALE

This procedure stops a science run in progress if necessary and then executes the SOP which loads the Standard Rev A and Optional Rev A patches. This is followed by the SOP to restart DEA housekeeping.

RESTRICTIONS/WARNINGS/NOTES/SCHEDULE REQT:

STEP INSTRUCTIONS (Command/Script) RESPONSE (TLM Verifier) 1 Uplink Loads:

1A AA000 191.CLD 502066E 2 Enable and Activate SCS 191, if necessary stopScience (command ID = 1539) 3 ACIS confirms proper execution of command 3 Execute SOP 61007 SW EVHCC3X3 4 ACIS confirms ACIS is restored to

default configuration.

5 Clear and disable SCS 191 6 Execute SOP 61010 DEA HKP 7 ACIS confirms existence of DEA HKP data

Approved:

Subsystem Engineer: Flight Director: TST Manager/Lead: Program Manager: SOT Lead: