AXAF COMMAND ACTION PROCEDURE

CAP # 632 ORIGINATOR: Paul Plucinsky DATE: 13 July 2000 COMMANDS CHECKED BY: Time of CAP Execution (GMT): 195:18:15

DESCRIPTION/RATIONALE

This CAP is to put us in a position to run the Squeegy CAP 625B in recovery from the high radiation environment on day 195. ACIS will decide to run IF the instaneous EPHIN P4 rate is less than and steady at 1000 counts/sample and the E1300 rate is less than and steady at 400 counts/sample.

ffl Enable RADMON

ffl Enable SCS 107

RESTRICTIONS/WARNINGS/NOTES/SCHEDULE REQT:

STEP INSTRUCTIONS (Command/Script) RESPONSE (TLM Verifier) EXECUTE:

1 Enable RADMON OC/CC verifies 2 Enable SCS 107 OC/CC verifies 3 Run CAP625B Squeegy R7

Approved:

Subsystem Engineer: Flight Director: TST Manager/Lead: Program Manager: SOT Lead: