AXAF COMMAND ACTION PROCEDURE

CAP # 636 ORIGINATOR: Paul Plucinsky DATE: 14 July 2000 COMMANDS CHECKED BY: Time of CAP Execution (GMT): 196:23:00

DESCRIPTION/RATIONALE

This CAP issues one command to power down the FEPs because of the high radiation environment on day 196.

RESTRICTIONS/WARNINGS/NOTES/SCHEDULE REQT:

STEP INSTRUCTIONS (Command/Script) RESPONSE (TLM Verifier) EXECUTE:

1 Uplink Load:

1A WS003 165.CLD 8121972 2 Enable and Activate SCS 165 WSFEPALLDN (cmdId = 1542) 3 clear and disable SCS 165

Approved:

Subsystem Engineer: Flight Director: TST Manager/Lead: Program Manager: SOT Lead: