AXAF COMMAND ACTION PROCEDURE

CAP #: 894 ORIGINATOR: Nancy Adams-Wolk DATE: 03 Nov 2003 COMMANDS CHECKED BY: Time of CAP Execution (GMT): 307:19:45

DESCRIPTION/RATIONALE

Warmboot the ACIS BEP and (re-) start a DEA Hkp Run after the SCS 107 execution on Day 306. The ACIS BEP had a watchdog reboot, presumably because the video boards were powered down while the FEPs were still acquiring/computing their bias maps.

RESTRICTIONS/WARNINGS/NOTES/SCHEDULE REQT:

FMT 2 needed. Since the daily load is suspended, there should be no conflicts with this commanding.

STEP INSTRUCTIONS (Command/Script) RESPONSE (TLM Verifier) EXECUTE:

1 SOP 61070 Warm Boot BEP ACIS verifies 2 SOP 61010 Start DEA Hkp ACIS verifies

Approved:

Subsystem Engineer: Flight Director: TST Manager/Lead: Program Manager: SOT Lead: