Table 1: FOT Flight Procedure Release on March 10, 1999 # Title Filenames SOP name New PB 1.1 1.0 Open Little Vent Valve open lvv MZ 61031 LIT VV ppp.txt 1.2 V1.0 Monitor Pressures and Temps monitor tp MZ 61017 MONITOR TEMP ppp.txt during Orbital Insertion 1.3 V1.0 Turn on DPA A & B and DEA A turnon dpaab deaa MZ 61002 DPA ON ppp.txt 1.4 V1.0 Load DEA HK PB and deahkp MZ 61010 DEA HKP ppp.txt Start DEA HK Run 1.5 V1.0 Turn on the DA Heater Side B dahtr b on MZ 61014 FBO HTR ppp.txt 1.6 V1.0 Set FP Temperature to -120 C setFP m120 MZ 61015 FBO TMP ppp.txt 1.7 V1.0 Open Large Vent Valve open vv MZ 61006 LRG VV ppp.txt 1.9 V1.0 Set FP Temperature to -90 C setFP m90 MZ 61030 FPTEMP NEG90 ppp.txt 1.10 V1.0 Dump Flight SW fs dump MZ 61055 DUMP FSW ppp.txt 1.13 V1.0 Diagnostic Mode ccd diag MZ 61024 DIAG MODE SCS ppp.txt 1.14 V1.0 Raw Data from each CCD ccd raw MZ 61054 RAW DATA CCD ppp.txt Y 1.20 V1.0 Flight SW: Event Histogram patch sw evhpatch MZ 61058 SWP EVH ppp.txt 1.21 V1.0 Evt Hist on the Int Cal Source ccd evhist s MZ 61012 EVH CAL ACIS-S ppp.txt Y with ACIS-S in fmt 1 2.3 V1.0 SW Boot Modes: Uplink Boot uplink boot MZ 61022 SW BOOT UPLINK ppp.txt 2.4 V1.0 SW Boot Modes: Warm and Cold swbootmode MZ 61023 SW BOOT WC ppp.txt 2.5 V1.0 BEP/DEA Power Combinations power combo MZ 61019 POWER COMBO ppp.txt 2.6 V1.0 DEA/FEP MUX Verification deafep mux MZ 61008 DEA FEP MUX ppp.txt 2.9 V1.0 Full Bakeout full bakeout cold MZ 61005 FULL BO ppp.txt 4.9 V1.0 Turn Off DPA A & B and DEA A turnoff dpaab deaa MZ 61011 DPA OFF ppp.txt 4.10 V1.0 Put ACIS into Memory Save Mode mem save MZ 61016 MEMORY SAVE ppp.txt 4.11 V1.0 Put ACIS into Standby Mode standby MZ 61021 STANDBY MODE ppp.txt