\documentstyle[11pt]{article}

\thispagestyle{empty}

\begin{document}


{\bf Definitive List of Columns in tab-separated ASCII files for ACIS
command procedures.}

\begin{tabbing}
Col	\=TLM Description \=value like 1.0,1.1,1.2 indicating step in the procedure \kill
Col	\>Title		  \>Description  \\
1	\>Step \#	  \>value like 1.0,1.1,1.2 indicating step in the procedure \\
2	\>Title		  \> \\
3	\>Time		  \>Predicted elasped time to execute step and verify \\
	\>		  \>if required, in minutes \\
4	\>CMD Description \>Text from IP\&CL which will appear on SOT
ACIS screens \\
5	\>CMD Mnemonic	  \>ACIS command mnemonics from IP\&CL or Ford's SW \\
	\>		  \> command mnemonic memo \\
6	\>CMD EGSE	  \>Text on ACIS EGSE SW \\
7	\>Sequence Key	  \>Name of command sequence in the ODB \\
8	\>TLM Description \>Text from IP\&CL which will appear on SOT
ACIS screens \\
9	\>TLM Mnemonic	  \>ACIS telemetry mnemonics from IP\&CL or SW telemetry \\
	\>		  \>structures \\
10	\>Expected Value  \>Value of HW telemetry verifier \\
11	\>Units		  \>units of verifier	 \\
12	\>TLM EGSE	  \>Text on ACIS EGSE SW \\
13	\>Other Verifier  \>Other HW or SW telemetry values which verify proper \\
	\>		  \>execution \\
14	\>Criticality	  \>1: HW verifier must have right value to proceed \\
	\>		  \>2: Expect HW verifier to have correct value but \\
	\>		  \>proceed regardless \\
	\>		  \>A: SW telemetry must have correct format to proceed \\
	\>		  \>B: Expect SW telemetry to have correct format but \\
	\>		  \>proceed regardless \\
	\>		  \>Blank: proceed without any verification \\
15	\>Description	  \>Additional text describing purpose or execution of \\
	\>		  \>step \\
16	\>Notes		  \>Footnotes for references or additional discussion \\
17	\>RT Con	  \>Real-time contact rewquired, either Y or blank for No \\
18	\>TLM Fmt	  \>TLM format required to execute step \\
19	\>Min Alt	  \>Required minimum altitude in thousands of km \\
20	\>SIM Pos	  \>Required SIM position, ACIS-I, ACIS-S, HRC-I, HRC-S \\

\end{tabbing}

The last row in the file will include a value for the total time
computed by summing the entries in column \#3 above.


\end{document}
