1.4 V2.0 LOAD DEA HK PB AND START DEA HK RUN

Last Revised: June 23,1999 Filename: dea hkp

BRIEF FUNCTIONAL DESCRIPTION:

This is an “atomic” procedure which simply loads a DEA Housekeeping parameter block and starts a DEA Housekeeping run.

The sequence of actions will be:

1. load the DEA Housekeeping PB 2. start the DEA Housekeeping run

ASSUMED INSTRUMENT STATE:

Assumes that at least one side of the DPA and DEA A are on and the flight SW is running.

SPECIAL INITIAL CONDITIONS:

OPERATIONAL CONSTRAINTS/CAUTIONS:

REFERENCES:

CHANGE HISTORY:

V1.2

ffl changed filenames from “deahkp” to “dea hkp”

V1.3

ffl moved TLM verifiers from “Telemetry Description” column to “Telemetry EGSE” column ffl changed required TLM format to 1 or 2 ffl changed criticality in step 2 to “B” and removed request for realtime contact ffl waiting for Bob’s crib sheet of DEA HKP values to check ffl deleted “CMD EGSE” and “SEQ KEY” from the LaTeX table

V1.4

ffl added the “commandEcho” values for the SW command packets ffl added filename identification to top of procedure

V2.0

ffl ACIS Team signed-off version, identical to previous version 1.4

Table 1: LOAD DEA HK PB AND START DEA HK RUN Step Title Time Command Command Telemetry Telemetry Expected Units # (Revision 1.4 V2.0) Req (m) Description Mnemonic Description Mnemonic Value 1.0 Execute DEA HK run 1.1 Load Board 11 DEA HK 1 loadDeaBlock WD00001024

1.2 Start DEA Hkp run 1 startDEA XDZ0000005

Total Time 2

Table 2: (CONT) LOAD DEA HK PB AND START DEA HK RUN Step Telemetry Other Crit Description Notes RT Tlm Min SIM # EGSE Verifier Con Fmt Alt Pos 1.0 1.1 Check cmdResult == OK B Load Fullhouse DEA housekeeping 1or2 commandEcho 225 parameter block into slot 4 1.2 deaHousekeepingData B get FP temp, should be stable and �2 C of desired value 1or2 commandEcho 18