\documentclass[11pt]{article}

\usepackage{lscape}

\topmargin -0.75truein
\oddsidemargin -0.4truein
\textheight 9.25truein
\textwidth 6.7truein
\hbadness=10001
\hfuzz=200pt


\begin{document}
%\input dspace12.tex
%\input pstricks.tex
%\input psfig
\newcommand{\be}{\begin{enumerate}}
\newcommand{\ee}{\end{enumerate}}
\newcommand{\bc}{\begin{center}}
\newcommand{\ec}{\end{center}}
\newcommand{\bi}{\begin{itemize}}
\newcommand{\ei}{\end{itemize}}
\newcommand{\bd}{\begin{description}}
\newcommand{\ed}{\end{description}}
\newcommand{\bt}{\begin{tabbing}}
\newcommand{\et}{\end{tabbing}}
\newcommand{\eg}{{\it e.g.~}}
\newcommand{\ie}{{\it i.e.~}}
\newcommand{\ul}{\underline}
\newcommand{\axaf}{{\em AXAF}}
\def\la{\hbox{\rlap{$<$}\lower0.5ex\hbox{$\sim$}\ }}


\large
%\vspace*{-0.5in}
\centerline {\bf 1.4\_V2.0 LOAD DEA HK PB AND START DEA HK RUN }
\vspace{0.25in}


\normalsize
\noindent{\it Last Revised: June 23,1999}\\
\noindent{\bf Filename: dea\_hkp} \\


\noindent {\bf BRIEF FUNCTIONAL DESCRIPTION:} \\
\normalsize
This is an ``atomic'' procedure which simply loads a DEA Housekeeping
parameter block and starts a DEA Housekeeping run.

\vspace{0.25in}
\noindent The sequence of actions will be: 
\be
\item load the DEA Housekeeping PB 
\vspace{-0.10in}
\item start the DEA Housekeeping run
\ee


\vspace{0.15in}
\normalsize
\noindent {\bf ASSUMED INSTRUMENT STATE:} \\
\normalsize
Assumes that at least one side of the DPA and DEA A are on and the
flight SW is running. \\


%\vspace{0.25in}
\normalsize
\noindent {\bf SPECIAL INITIAL CONDITIONS:} \\
\normalsize
%The environment must be clean enough to allow opening of the valve. \\
%Assumes that \axaf\/ ISIM RCTU is powered on and in telemetry format 6. \\

%\newpage 

%\vspace{0.25in}
\normalsize
\noindent {\bf OPERATIONAL CONSTRAINTS/CAUTIONS:} \\
\normalsize



\vspace{0.15in}
\normalsize
\noindent {\bf REFERENCES:} \\
\normalsize

\normalsize
\noindent {\bf CHANGE HISTORY:} \\
\normalsize

{\bf V1.2}
\begin{itemize}
\item changed filenames from ``deahkp'' to ``dea\_hkp''
\end{itemize}

{\bf V1.3}
\begin{itemize}
\item moved TLM verifiers from ``Telemetry Description'' column to
``Telemetry EGSE'' column 
\item changed required TLM format to 1 or 2
\item changed criticality in step 2 to ``B'' and removed request for
realtime contact
\item waiting for Bob's crib sheet of DEA HKP values to check
\item deleted ``CMD EGSE'' and ``SEQ KEY'' from the LaTeX table
\end{itemize}

{\bf V1.4}
\begin{itemize}
\item added the ``commandEcho'' values for the SW command packets
\item added filename identification to top of procedure
\end{itemize}

{\bf V2.0}
\begin{itemize}
\item ACIS Team signed-off version, identical to previous version 1.4
\end{itemize}

\newcommand{\tablecaptiontext}{LOAD DEA HK PB AND START DEA HK RUN}
\input{dea_hkp.tab}

\end{document}

