\documentclass[11pt]{article}

\usepackage{lscape}

\topmargin -1.0truein
\oddsidemargin -0.5truein
\textheight 9.75truein
\textwidth 7.0truein
\hbadness=10001
\hfuzz=200pt



\begin{document}


\begin{landscape}

\begin{table}[tbp]
\centering
\caption[ ]{\bf Renaming of ACIS SOT Procedure Filenames April 21, 1999}

\begin{tabular}{|l|l|l|l|l|}
\hline
Old \#  & Title		& Old Filenames & New \# & New Filenames  \\
\hline
\hline
1.1\_V1.1 & Open Little Vent Valve & open\_lvv & 1.1\_V1.2 & open\_svv \\
\hline
1.2\_V1.1 & Monitor Pressures and Temps & monitor\_tp & No change & same \\
          & during Orbital Insertion & & &   \\
\hline
1.3\_V1.1 & Turn on DPA A \& B and DEA A & turnon\_dpaab\_deaa & 1.3\_V1.3  & dpaab\_deaa\_on  \\
\hline
1.4\_V1.1 & Load DEA HK PB and  & deahkp  & 1.4\_V1.2 & dea\_hkp \\
          & Start DEA HK Run & & & \\
\hline
1.5\_V1.1 & Turn on the DA Heater Side B & dahtr\_b\_on & no change & same  \\
\hline
1.6\_V1.1 & Set FP Temperature to -120~C & setFP\_m120 & 1.6\_V1.2,name change  & setfp\_m120  \\
\hline
1.7\_V1.1 & Open Large Vent Valve & open\_vv & 1.7\_V1.2  & open\_bvv  \\
\hline
1.9\_V1.1 & Set FP Temperature to -90 C & setFP\_m90  & 1.9\_V1.2,name
change & setfp\_m90 \\
\hline
1.10\_V1.1 & Dump Flight SW & fs\_dump & 1.10\_V1.2 & sw\_dump \\
\hline
1.13\_V1.1 & Diagnostic Mode & ccd\_diag\_posttv & 1.13\_V1.2  & diag\_scs  \\
\hline
1.14\_V1.1 & Raw Data from each CCD & ccd\_raw & 1.14\_V1.2,name change & raw\_data   \\
\hline
1.20\_V1.1 & Flight SW: Event Histogram patch & sw\_evhpatch &
1.20\_V1.2 & same  \\
\hline
1.21\_V1.1 & Evt Hist on the Int Cal Source  & ccd\_evhist\_s &
1.21\_V1.2  & evhist\_sarray  \\
           & with ACIS-S in fmt 1 & & &  \\
\hline
2.3\_V1.1 & SW Boot Modes: Uplink Boot & uplink\_boot & 2.3\_V1.2 & same \\
\hline
2.4\_V1.1 & SW Boot Modes: Warm and Cold & swbootmode & 2.4\_V1.2 & same \\
\hline
2.5\_V1.1 & BEP/DEA Power Combinations & power\_combo & 2.5\_V1.2 & same \\
\hline
2.6\_V1.1 & DEA/FEP MUX Verification & deafep\_mux & 2.6\_V1.2 & same  \\
\hline
2.9\_V1.1 & Full Bakeout & full\_bakeout\_cold & 2.9\_V1.2,name change & full\_bakeout \\
\hline
4.9\_V1.1 & Turn Off DPA A \& B and DEA A & turnoff\_dpaab\_deaa  &
4.9\_V1.2 & dpaab\_deaa\_off  \\
\hline
4.10\_V1.1 & Put ACIS into Memory Save Mode & mem\_save & No change & same  \\
\hline
4.11\_V1.1 & Put ACIS into Standby Mode   & standby & No change & same  \\
\hline
\end{tabular}

\end{table}

\end{landscape}

\newpage 

\begin{landscape}

\begin{table}[tbp]
\centering
%\caption[ ]{\bf FOT Flight Procedure Release on March 19, 1999}
\caption[ ]{\bf Renaming of ACIS SOT Procedure Filenames April 24,
1999}

\begin{tabular}{|l|l|l|l|l|}
\hline
Old \#  & Title		& Old Filenames & New \# & New Filenames  \\
\hline
\hline
4.19\_V1.1 & Radiation Belt Entry  & radbelt\_entry & no change  & same \\
\hline
1.8\_V1.1 & Partial Bakeout, set FP to -50 C & bakeout\_m50C &
1.8\_V1.2,name change & bakeout\_m50 \\
\hline
1.11\_V1.1 & Flight Software Standard Set of Patches (realtime) &
sw\_stdpatch & not reviewed  & same  \\
\hline
1.12\_V1.1 & Flight Software Event Histogram and CC 3x3 Patch &
sw\_optevhcc3x3 & 1.12\_V1.2,name change & sw\_evhcc3x3  \\
\hline
1.15\_V1.1 & OBF Integrity Test & ccd\_obf & 1.15\_V1.2,name change  & obf\_intg \\
\hline
1.16\_V1.1 & Dark Current Measurement & ccd\_dark & 1.16\_V1.2,name change  & dark\_cur  \\
\hline
1.17\_V1.1 &  Internal Calibration Source Measurement at -90~C &
ccd\_int1 & 1.17\_V1.2,name change  & intcal\_m90  \\
\hline
1.18\_V1.1  & Internal Calibration Source Measurement at -110~C &
ccd\_int2 & 1.18\_V1.2,name change & intcal\_m110  \\
\hline
1.19\_V1.1  & Internal Calibration Source Measurement at -120~C &
ccd\_int3 & 1.19\_V1.2,name change & intcal\_m120  \\
\hline
2.2\_V1.1 & Exercise Focal Plane Heater Controls & heater\_fp & not
reviewed  & same  \\
\hline
2.7\_V1.1 & DEA Video Board DAC Limit Test & dac\_limits & not reviewed & same  \\
\hline
2.8\_V1.1  & CCD Orbital Background Measurements & ccd\_orbbkg1 & 2.8\_V1.2,name change & bkg\_doorcl \\
\hline
2.11\_V1.1 & CCD Orbital Background Measurements II & ccd\_orbbkg2 & 2.11\_V1.2,name change &
bkg\_doorop   \\
\hline
2.12\_V1.1  & HRMA Flux Standard Transfer Sources Measurements &
ccd\_fcm & 2.12\_V1.2,name change & hrma\_fcm  \\
\hline
4.2\_V1.1  & Turn on DPA A \& B and DEA A [SCS version] &
turnon\_dpaab\_deaa\_scs & 4.2\_V1.2  & dpaab\_deaa\_scs \\
\hline
4.3\_V1.1  & Turn on DPA A  & turnon\_dpaa & 4.3\_V1.2 & dpaa\_on \\
\hline
4.4\_V1.1  & Turn on DPA B  & turnon\_dpab & 4.4\_V1.2 & dpab\_on \\
\hline
4.5\_V1.1  & Turn on DEA A  & turnon\_deaa & 4.5\_V1.2 & deaa\_on \\
\hline
4.6\_V1.1  & Turn off DPA A & turnoff\_dpaa & 4.6\_V1.2 & dpaa\_off \\
\hline
4.7\_V1.1  & Turn off DPA B & turnoff\_dpab & 4.7\_V1.2 & dpab\_off \\
\hline
4.8\_V1.1  & Turn off DEA A & turnoff\_deaa & 4.8\_V1.2 & deaa\_off \\
\hline
4.15\_V1.1 & Set focal plane temperature to -50 C & setFP\_m50 &
4.15\_V1.2,name change & setfp\_m50 \\
\hline
4.17\_V1.1 & Warm Boot the ACIS BEP & warmboot & no change & same\\
\hline
4.18\_V1.1 & Cold Boot the ACIS BEP & coldboot & no change & same \\
\hline
5.1\_V1.1 & Close Little Vent Valve & close\_lvv & 5.1\_V1.2,name change & close\_svv \\
\hline
5.2\_V1.1 & Abort Opening Large Vent Valve & abort\_opvv & DELETED & \\
\hline
5.3\_V1.1 & Close Large Vent Valve & close\_vv & 5.3\_V1.3 & close\_bvv \\
\hline
5.4\_V1.1 & Abort Closing Large Vent Valve & abort\_clvv & DELETED &
 \\
\hline
5.5\_V1.1 & Open Little Vent Valve in Emergency Deployment  &
open\_lvv\_emgdep & 5.5\_1.2,name change & open\_svv\_emgdp  \\
          & [SCS version] & & & \\
\hline
5.6\_V1.1 & Turn Off DA heater side B and turn on side A &
dahtr\_aon\_boff & no change  & same  \\
\hline
5.7\_V1.1 & Turn Off DA heater side A and turn on side B &
dahtr\_bon\_aoff & no change & same \\
\hline
5.8\_V1.1 & Switch from BEP A to BEP B & switch\_bepa\_b & 5.8\_V1.2 & same  \\
\hline
5.9\_V1.1 & Switch from DEA A to DEA B & switch\_deaa\_b & not
reviewed & same  \\
\hline
\end{tabular}

\end{table}

\end{landscape}

\end{document}




\end{document}

