\documentclass[11pt]{article}

\usepackage{lscape}

\topmargin -0.75truein
\oddsidemargin -0.0truein
\textheight 9.5truein
\textwidth 6.7truein
\hbadness=10001
\hfuzz=200pt


\begin{document}
%\input dspace12.tex
%\input pstricks.tex
%\input psfig
\newcommand{\be}{\begin{enumerate}}
\newcommand{\ee}{\end{enumerate}}
\newcommand{\bc}{\begin{center}}
\newcommand{\ec}{\end{center}}
\newcommand{\bi}{\begin{itemize}}
\newcommand{\ei}{\end{itemize}}
\newcommand{\bd}{\begin{description}}
\newcommand{\ed}{\end{description}}
\newcommand{\bt}{\begin{tabbing}}
\newcommand{\et}{\end{tabbing}}
\newcommand{\eg}{{\it e.g.~}}
\newcommand{\ie}{{\it i.e.~}}
\newcommand{\ul}{\underline}
\newcommand{\axaf}{{\em AXAF}}
\def\la{\hbox{\rlap{$<$}\lower0.5ex\hbox{$\sim$}\ }}


\large
%\vspace*{-0.5in}
\centerline {\bf 2.15\_V1.0 RAW MODE DATA IN POSTAGE STAMP FORMAT}
\vspace{0.25in}

\normalsize
\noindent{\it Last Revised: August 10, 1999}\\
\noindent{\bf Filename: raw\_stamp} \\

\noindent {\bf BRIEF FUNCTIONAL DESCRIPTION:} \\
\normalsize

This procedure uses subarray format and windows to telemeter quickly
100\,x\,100-pixel raw sub-images centered on the middle of quadrant D
of CCD I3.  These data will be analyzed for particles and compared to
the event rates from the EPHIN instrument.

\vspace{0.25in}
\noindent The sequence of actions will be: 
\be
\item start a DEA HKP run if necessary
\vspace{-0.10in}
\item configure the instrument to collect imaging array data with 6 video
boards up, but only 1 FEP attached to a DEA board
\vspace{-0.10in}
\item execute the science run, collect an hour or two of raw sub-frames from CCD I3, including a dump of all the configuration information
\vspace{-0.10in}
\item reconfigure back to the thermal standby state if necessary
\vspace{-0.10in}
\ee


\vspace{0.15in}
\normalsize
\noindent {\bf ASSUMED INSTRUMENT STATE:} \\
\normalsize
Assumes the instrument is in the canonical thermal standby state.\\
Assumes the standard patches are loaded.\\

%\vspace{0.25in}
\normalsize
\noindent {\bf SPECIAL INITIAL CONDITIONS:} \\
\normalsize

%\newpage 

%\vspace{0.25in}
\normalsize
\noindent {\bf OPERATIONAL CONSTRAINTS/CAUTIONS:} \\
\normalsize
Assumes the spacecraft is in TLM FMT 2 throughout the procedure to telemeter the raw frames in a reasonable amount of time.\\

\vspace{0.25in}
\normalsize
\noindent {\bf SPECIAL FINAL CONDITIONS:} \\
\normalsize


%\vspace{0.15in}
\normalsize
\noindent {\bf REFERENCES:} \\
\normalsize
\be
\item MIT 36-58010, Standard Patch Release, Rev. A
\ee


\vspace{0.15in}
\normalsize
\noindent {\bf CHANGE HISTORY:} \\
\normalsize

{\bf V1.0}
\begin{itemize}
\item Initial version, copied from procedure 1.27\_V2.1 ``Raw Mode Data
  for Bias Algorithm Optimization''.
\item Revised the procedure title, date, and filename
\item Revised the brief functional description
\item Revised the sequence of actions
\item Set command mnemonic to ``WT00175014'' and command echo to ``1379''
in step 3.1
\item Set command mnemonic to ``W200030014'' and command echo to ``1369''
\item Revised time required field to 120 min in step 3.15
\item Revised time required fiels to 5 min in step 3.17
in step 3.2

\end{itemize}

\newcommand{\tablecaptiontext}{Collect Raw Mode Data in Postage Stamp Format}
\input{raw_stamp.tab}

\end{document}
