\documentclass[11pt]{article}

\usepackage{lscape}

\topmargin -0.75truein
\oddsidemargin -0.3truein
\textheight 9.25truein
\textwidth 7.3truein
\hbadness=10001
\hfuzz=200pt


\begin{document}
%\input dspace12.tex
%\input pstricks.tex
%\input psfig
\newcommand{\be}{\begin{enumerate}}
\newcommand{\ee}{\end{enumerate}}
\newcommand{\bc}{\begin{center}}
\newcommand{\ec}{\end{center}}
\newcommand{\bi}{\begin{itemize}}
\newcommand{\ei}{\end{itemize}}
\newcommand{\bd}{\begin{description}}
\newcommand{\ed}{\end{description}}
\newcommand{\bt}{\begin{tabbing}}
\newcommand{\et}{\end{tabbing}}
\newcommand{\eg}{{\it e.g.~}}
\newcommand{\ie}{{\it i.e.~}}
\newcommand{\ul}{\underline}
\newcommand{\axaf}{{\em AXAF}}
\def\la{\hbox{\rlap{$<$}\lower0.5ex\hbox{$\sim$}\ }}


\large
%\vspace*{-0.5in}
\centerline {\bf 4.20\_V2.0 TURN OFF PRESSURE TRANSDUCERS A \& B}

\vspace{0.25in}

\normalsize
\noindent{\it Last Revised: June 23,1999}\\
\noindent{\bf Filename: xdcr\_ab\_off} \\

\noindent {\bf BRIEF FUNCTIONAL DESCRIPTION:} \\
\normalsize

This is an atomic procedure which simply turns off the pressure
transducers.


\vspace{0.25in}
\noindent The sequence of actions will be: 
\be
\item turn off the pressure transducer A \& B, check the pressure to
ensure the transducers are off
\ee


\vspace{0.15in}
\normalsize
\noindent {\bf ASSUMED INSTRUMENT STATE:} \\
\normalsize
Assumes that the PSMC has power from the spacecraft. \\

%\vspace{0.25in}
\normalsize
\noindent {\bf SPECIAL INITIAL CONDITIONS:}\\
\normalsize
Assumes that \axaf\/ ISIM RCTU is powered on and in telemetry
format 1, 2, or 4. \\

%\newpage 

%\vspace{0.25in}
\normalsize
\noindent {\bf OPERATIONAL CONSTRAINTS/CAUTIONS:} \\
\normalsize
ACIS-C-002 \\


%\vspace{0.15in}
\normalsize
\noindent {\bf REFERENCES:} \\
\normalsize

\normalsize
\noindent {\bf CHANGE HISTORY:} \\
\normalsize

{\bf V2.0}
\begin{itemize}
\item ACIS Team signed-off version
\item changed required telemetry format to 1,2,4 or 6
\item added units of minutes (m) to the Time Req column
\end{itemize}


\newcommand{\tablecaptiontext}{Turn off Pressure Transducers A \& B}
\input{xdcr_ab_off.tab}

\end{document}


